sis> UC Berkeley, SIS 1.3.6 (compiled 2007-07-18 12:59:37)
sis> <-- START --> 
sis> sis> <-- bbara --> 
sis> sis> jedi_output   	pi= 4	po= 2	nodes=  5	latches= 3
lits(sop)=  93	#states(STG)=   7
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 459.8 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- bbsse --> 
sis> sis> jedi_output   	pi= 7	po= 7	nodes= 11	latches= 4
lits(sop)= 280	#states(STG)=  13
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 1044.7 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- bbtas --> 
sis> sis> jedi_output   	pi= 2	po= 2	nodes=  5	latches= 3
lits(sop)=  54	#states(STG)=   6
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 270.6 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- beecount --> 
sis> sis> jedi_output   	pi= 3	po= 4	nodes=  6	latches= 2
lits(sop)=  83	#states(STG)=   4
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 376.5 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- cse --> 
sis> sis> jedi_output   	pi= 7	po= 7	nodes= 11	latches= 4
lits(sop)= 701	#states(STG)=  16
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 2087.3 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- dk14 --> 
sis> sis> jedi_output   	pi= 3	po= 5	nodes=  8	latches= 3
lits(sop)= 346	#states(STG)=   7
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 1199.9 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- dk15 --> 
sis> sis> jedi_output   	pi= 3	po= 5	nodes=  7	latches= 2
lits(sop)= 213	#states(STG)=   4
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 790.6 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- dk16 --> 
sis> sis> jedi_output   	pi= 2	po= 3	nodes=  8	latches= 5
lits(sop)= 636	#states(STG)=  27
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 2315.5 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- dk17 --> 
sis> sis> jedi_output   	pi= 2	po= 3	nodes=  6	latches= 3
lits(sop)= 129	#states(STG)=   8
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 607.2 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- dk27 --> 
sis> sis> jedi_output   	pi= 1	po= 2	nodes=  5	latches= 3
lits(sop)=  28	#states(STG)=   7
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 204.6 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- ex1 --> 
sis> sis> jedi_output   	pi= 9	po=19	nodes= 24	latches= 5
lits(sop)= 859	#states(STG)=  18
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 2812.4 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- ex3 --> 
sis> sis> jedi_output   	pi= 2	po= 2	nodes=  5	latches= 3
lits(sop)=  43	#states(STG)=   5
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 273.8 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- ex4 --> 
sis> sis> jedi_output   	pi= 6	po= 9	nodes= 13	latches= 4
lits(sop)= 170	#states(STG)=  14
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 794.4 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- ex5 --> 
sis> sis> jedi_output   	pi= 2	po= 2	nodes=  4	latches= 2
lits(sop)=  30	#states(STG)=   4
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 194.2 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- ex6 --> 
sis> sis> jedi_output   	pi= 5	po= 8	nodes= 11	latches= 3
lits(sop)= 419	#states(STG)=   8
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 1446.0 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- ex7 --> 
sis> sis> jedi_output   	pi= 2	po= 2	nodes=  4	latches= 2
lits(sop)=  54	#states(STG)=   4
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 293.4 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- keyb --> 
sis> sis> jedi_output   	pi= 7	po= 2	nodes=  7	latches= 5
lits(sop)= 544	#states(STG)=  19
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 1721.4 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- lion9 --> 
sis> sis> jedi_output   	pi= 2	po= 1	nodes=  3	latches= 2
lits(sop)=  20	#states(STG)=   4
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 143.2 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- lion --> 
sis> sis> jedi_output   	pi= 2	po= 1	nodes=  3	latches= 2
lits(sop)=  21	#states(STG)=   4
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 159.5 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- mark1 --> 
sis> sis> jedi_output   	pi= 5	po=16	nodes= 20	latches= 4
lits(sop)= 293	#states(STG)=  12
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 982.7 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- mc --> 
sis> sis> jedi_output   	pi= 3	po= 5	nodes=  7	latches= 2
lits(sop)=  71	#states(STG)=   4
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 312.2 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- opus --> 
sis> sis> jedi_output   	pi= 5	po= 6	nodes= 10	latches= 4
lits(sop)= 269	#states(STG)=   9
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 1014.4 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- planet1 --> 
sis> sis> jedi_output   	pi= 7	po=19	nodes= 25	latches= 6
lits(sop)=2648	#states(STG)=  48
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 7687.9 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- planet --> 
sis> sis> jedi_output   	pi= 7	po=19	nodes= 25	latches= 6
lits(sop)=2648	#states(STG)=  48
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 7687.9 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- s1488 --> 
sis> sis> jedi_output   	pi= 8	po=19	nodes= 25	latches= 6
lits(sop)=2415	#states(STG)=  48
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 6958.5 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- s1494 --> 
sis> sis> jedi_output   	pi= 8	po=19	nodes= 25	latches= 6
lits(sop)=2291	#states(STG)=  48
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 6628.0 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- s1 --> 
sis> sis> jedi_output   	pi= 8	po= 6	nodes= 11	latches= 5
lits(sop)= 468	#states(STG)=  20
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 1369.9 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- s208 --> 
sis> sis> jedi_output   	pi=11	po= 2	nodes=  7	latches= 5
lits(sop)= 188	#states(STG)=  18
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 721.0 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- s27 --> 
sis> sis> jedi_output   	pi= 4	po= 1	nodes=  4	latches= 3
lits(sop)=  72	#states(STG)=   5
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 365.1 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- s298 --> 
sis> sis> jedi_output   	pi= 3	po= 6	nodes= 14	latches= 8
lits(sop)=6594	#states(STG)= 135
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 17399.6 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- s386 --> 
sis> sis> jedi_output   	pi= 7	po= 7	nodes= 11	latches= 4
lits(sop)= 437	#states(STG)=  13
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 1414.4 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- s420 --> 
sis> sis> jedi_output   	pi=19	po= 2	nodes=  7	latches= 5
lits(sop)= 249	#states(STG)=  18
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 857.7 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- s510 --> 
sis> sis> jedi_output   	pi=19	po= 7	nodes= 13	latches= 6
lits(sop)= 892	#states(STG)=  47
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 3158.6 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- s820 --> 
sis> sis> jedi_output   	pi=18	po=19	nodes= 24	latches= 5
lits(sop)= 925	#states(STG)=  24
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 2939.3 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- s832 --> 
sis> sis> jedi_output   	pi=18	po=19	nodes= 24	latches= 5
lits(sop)= 884	#states(STG)=  24
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 2824.4 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- sand --> 
sis> sis> jedi_output   	pi=11	po= 9	nodes= 15	latches= 6
lits(sop)=2729	#states(STG)=  32
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 6905.2 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- shiftreg --> 
sis> sis> jedi_output   	pi= 1	po= 1	nodes=  4	latches= 3
lits(sop)=  18	#states(STG)=   8
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 148.8 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- sse --> 
sis> sis> jedi_output   	pi= 7	po= 7	nodes= 11	latches= 4
lits(sop)= 280	#states(STG)=  13
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 1044.7 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- styr --> 
sis> sis> jedi_output   	pi= 9	po=10	nodes= 15	latches= 5
lits(sop)=1837	#states(STG)=  30
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 5284.7 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- tav --> 
sis> sis> jedi_output   	pi= 4	po= 4	nodes=  6	latches= 2
lits(sop)=  35	#states(STG)=   4
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 200.9 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- tbk --> 
sis> sis> jedi_output   	pi= 6	po= 3	nodes=  7	latches= 4
lits(sop)= 887	#states(STG)=  16
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 2561.4 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- train11 --> 
sis> sis> jedi_output   	pi= 2	po= 1	nodes=  3	latches= 2
lits(sop)=  13	#states(STG)=   4
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 111.3 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- train4 --> 
sis> sis> jedi_output   	pi= 2	po= 1	nodes=  3	latches= 2
lits(sop)=  27	#states(STG)=   4
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 193.4 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
