sis> UC Berkeley, SIS 1.3.6 (compiled 2007-07-18 12:59:37)
sis> <-- START --> 
sis> sis> <-- bbara --> 
sis> sis> jedi_output   	pi= 4	po= 2	nodes=  5	latches= 3
lits(sop)= 146	#states(STG)=   7
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 584.9 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- bbsse --> 
sis> sis> jedi_output   	pi= 7	po= 7	nodes= 11	latches= 4
lits(sop)= 381	#states(STG)=  13
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 1343.1 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- bbtas --> 
sis> sis> jedi_output   	pi= 2	po= 2	nodes=  5	latches= 3
lits(sop)=  46	#states(STG)=   6
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 278.6 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- beecount --> 
sis> sis> jedi_output   	pi= 3	po= 4	nodes=  6	latches= 2
lits(sop)=  71	#states(STG)=   4
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 338.7 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- cse --> 
sis> sis> jedi_output   	pi= 7	po= 7	nodes= 11	latches= 4
lits(sop)= 806	#states(STG)=  16
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 2616.7 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- dk14 --> 
sis> sis> jedi_output   	pi= 3	po= 5	nodes=  8	latches= 3
lits(sop)= 398	#states(STG)=   7
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 1394.9 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- dk15 --> 
sis> sis> jedi_output   	pi= 3	po= 5	nodes=  7	latches= 2
lits(sop)= 181	#states(STG)=   4
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 703.5 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- dk16 --> 
sis> sis> jedi_output   	pi= 2	po= 3	nodes=  8	latches= 5
lits(sop)=1072	#states(STG)=  27
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 3486.4 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- dk17 --> 
sis> sis> jedi_output   	pi= 2	po= 3	nodes=  6	latches= 3
lits(sop)= 137	#states(STG)=   8
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 602.9 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- dk27 --> 
sis> sis> jedi_output   	pi= 1	po= 2	nodes=  5	latches= 3
lits(sop)=  47	#states(STG)=   7
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 310.2 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- ex1 --> 
sis> sis> jedi_output   	pi= 9	po=19	nodes= 24	latches= 5
lits(sop)=1336	#states(STG)=  18
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 4046.4 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- ex3 --> 
sis> sis> jedi_output   	pi= 2	po= 2	nodes=  5	latches= 3
lits(sop)=  50	#states(STG)=   5
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 324.4 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- ex4 --> 
sis> sis> jedi_output   	pi= 6	po= 9	nodes= 13	latches= 4
lits(sop)= 256	#states(STG)=  14
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 977.2 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- ex5 --> 
sis> sis> jedi_output   	pi= 2	po= 2	nodes=  4	latches= 2
lits(sop)=  48	#states(STG)=   4
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 280.4 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- ex6 --> 
sis> sis> jedi_output   	pi= 5	po= 8	nodes= 11	latches= 3
lits(sop)= 413	#states(STG)=   8
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 1500.3 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- ex7 --> 
sis> sis> jedi_output   	pi= 2	po= 2	nodes=  4	latches= 2
lits(sop)=  49	#states(STG)=   4
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 301.1 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- keyb --> 
sis> sis> jedi_output   	pi= 7	po= 2	nodes=  7	latches= 5
lits(sop)=1728	#states(STG)=  19
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 4763.0 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- lion9 --> 
sis> sis> jedi_output   	pi= 2	po= 1	nodes=  3	latches= 2
lits(sop)=  21	#states(STG)=   4
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 149.1 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- lion --> 
sis> sis> jedi_output   	pi= 2	po= 1	nodes=  3	latches= 2
lits(sop)=  21	#states(STG)=   4
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 159.5 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- mark1 --> 
sis> sis> jedi_output   	pi= 5	po=16	nodes= 20	latches= 4
lits(sop)= 340	#states(STG)=  12
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 1131.6 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- mc --> 
sis> sis> jedi_output   	pi= 3	po= 5	nodes=  7	latches= 2
lits(sop)=  84	#states(STG)=   4
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 367.8 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- opus --> 
sis> sis> jedi_output   	pi= 5	po= 6	nodes= 10	latches= 4
lits(sop)= 276	#states(STG)=   9
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 1007.0 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- planet1 --> 
sis> sis> jedi_output   	pi= 7	po=19	nodes= 25	latches= 6
lits(sop)=4197	#states(STG)=  48
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 10658.7 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- planet --> 
sis> sis> jedi_output   	pi= 7	po=19	nodes= 25	latches= 6
lits(sop)=4197	#states(STG)=  48
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 10658.7 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- s1488 --> 
sis> sis> jedi_output   	pi= 8	po=19	nodes= 25	latches= 6
lits(sop)=3030	#states(STG)=  48
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 8512.1 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- s1494 --> 
sis> sis> jedi_output   	pi= 8	po=19	nodes= 25	latches= 6
lits(sop)=3144	#states(STG)=  48
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 9023.9 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- s1 --> 
sis> sis> jedi_output   	pi= 8	po= 6	nodes= 11	latches= 5
lits(sop)=1703	#states(STG)=  20
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 5060.9 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- s208 --> 
sis> sis> jedi_output   	pi=11	po= 2	nodes=  7	latches= 5
lits(sop)= 203	#states(STG)=  18
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 819.6 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- s27 --> 
sis> sis> jedi_output   	pi= 4	po= 1	nodes=  4	latches= 3
lits(sop)=  78	#states(STG)=   5
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 388.4 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- s298 --> 
sis> sis> jedi_output   	pi= 3	po= 6	nodes= 14	latches= 8
lits(sop)=12748	#states(STG)= 135
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 34825.1 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- s386 --> 
sis> sis> jedi_output   	pi= 7	po= 7	nodes= 11	latches= 4
lits(sop)= 459	#states(STG)=  13
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 1603.6 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- s420 --> 
sis> sis> jedi_output   	pi=19	po= 2	nodes=  7	latches= 5
lits(sop)= 203	#states(STG)=  18
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 819.6 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- s510 --> 
sis> sis> jedi_output   	pi=19	po= 7	nodes= 13	latches= 6
lits(sop)=1800	#states(STG)=  47
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 5338.1 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- s820 --> 
sis> sis> jedi_output   	pi=18	po=19	nodes= 24	latches= 5
lits(sop)=1102	#states(STG)=  24
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 3379.6 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- s832 --> 
sis> sis> jedi_output   	pi=18	po=19	nodes= 24	latches= 5
lits(sop)=1220	#states(STG)=  24
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 3721.8 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- sand --> 
sis> sis> jedi_output   	pi=11	po= 9	nodes= 15	latches= 6
lits(sop)=3521	#states(STG)=  32
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 9396.0 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- shiftreg --> 
sis> sis> jedi_output   	pi= 1	po= 1	nodes=  4	latches= 3
lits(sop)=  56	#states(STG)=   8
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 325.0 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- sse --> 
sis> sis> jedi_output   	pi= 7	po= 7	nodes= 11	latches= 4
lits(sop)= 381	#states(STG)=  13
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 1343.1 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- styr --> 
sis> sis> jedi_output   	pi= 9	po=10	nodes= 15	latches= 5
lits(sop)=3304	#states(STG)=  30
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 8662.4 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- tav --> 
sis> sis> jedi_output   	pi= 4	po= 4	nodes=  6	latches= 2
lits(sop)=  35	#states(STG)=   4
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 200.9 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- tbk --> 
sis> sis> jedi_output   	pi= 6	po= 3	nodes=  7	latches= 4
lits(sop)= 941	#states(STG)=  16
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 2608.7 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- train11 --> 
sis> sis> jedi_output   	pi= 2	po= 1	nodes=  3	latches= 2
lits(sop)=  18	#states(STG)=   4
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 139.7 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- train4 --> 
sis> sis> jedi_output   	pi= 2	po= 1	nodes=  3	latches= 2
lits(sop)=  19	#states(STG)=   4
sis> Combinational power estimation, with Zero delay model.
Network: jedi_output, Power = 137.0 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
