sis> UC Berkeley, SIS 1.3.6 (compiled 2007-07-18 12:59:37)
sis> <-- START --> 
sis> sis> <-- bbara --> 
sis> sis> bbara.kiss2.esp	pi= 4	po= 2	nodes=  5	latches= 3
lits(sop)=  79	#states(STG)=   7
sis> Combinational power estimation, with Zero delay model.
Network: bbara.kiss2.esp, Power = 387.6 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- bbsse --> 
sis> sis> bbsse.kiss2.esp	pi= 7	po= 7	nodes= 11	latches= 4
lits(sop)= 299	#states(STG)=  13
sis> Combinational power estimation, with Zero delay model.
Network: bbsse.kiss2.esp, Power = 1055.3 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- bbtas --> 
sis> sis> bbtas.kiss2.esp	pi= 2	po= 2	nodes=  5	latches= 3
lits(sop)=  38	#states(STG)=   6
sis> Combinational power estimation, with Zero delay model.
Network: bbtas.kiss2.esp, Power = 230.1 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- beecount --> 
sis> sis> beecount.kiss2.esp	pi= 3	po= 4	nodes=  6	latches= 2
lits(sop)=  73	#states(STG)=   4
sis> Combinational power estimation, with Zero delay model.
Network: beecount.kiss2.esp, Power = 350.0 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- cse --> 
sis> sis> cse.kiss2.esp 	pi= 7	po= 7	nodes= 11	latches= 4
lits(sop)= 616	#states(STG)=  16
sis> Combinational power estimation, with Zero delay model.
Network: cse.kiss2.esp, Power = 1765.1 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- dk14 --> 
sis> sis> dk14.kiss2.esp	pi= 3	po= 5	nodes=  8	latches= 3
lits(sop)= 252	#states(STG)=   7
sis> Combinational power estimation, with Zero delay model.
Network: dk14.kiss2.esp, Power = 999.0 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- dk15 --> 
sis> sis> dk15.kiss2.esp	pi= 3	po= 5	nodes=  7	latches= 2
lits(sop)= 153	#states(STG)=   4
sis> Combinational power estimation, with Zero delay model.
Network: dk15.kiss2.esp, Power = 636.9 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- dk16 --> 
sis> sis> dk16.kiss2.esp	pi= 2	po= 3	nodes=  8	latches= 5
lits(sop)= 673	#states(STG)=  27
sis> Combinational power estimation, with Zero delay model.
Network: dk16.kiss2.esp, Power = 2386.9 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- dk17 --> 
sis> sis> dk17.kiss2.esp	pi= 2	po= 3	nodes=  6	latches= 3
lits(sop)= 128	#states(STG)=   8
sis> Combinational power estimation, with Zero delay model.
Network: dk17.kiss2.esp, Power = 572.6 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- dk27 --> 
sis> sis> dk27.kiss2.esp	pi= 1	po= 2	nodes=  5	latches= 3
lits(sop)=  33	#states(STG)=   7
sis> Combinational power estimation, with Zero delay model.
Network: dk27.kiss2.esp, Power = 236.7 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- ex1 --> 
sis> sis> ex1.kiss2.esp 	pi= 9	po=19	nodes= 24	latches= 5
lits(sop)= 910	#states(STG)=  18
sis> Combinational power estimation, with Zero delay model.
Network: ex1.kiss2.esp, Power = 3018.9 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- ex3 --> 
sis> sis> ex3.kiss2.esp 	pi= 2	po= 2	nodes=  5	latches= 3
lits(sop)=  41	#states(STG)=   5
sis> Combinational power estimation, with Zero delay model.
Network: ex3.kiss2.esp, Power = 269.1 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- ex4 --> 
sis> sis> ex4.kiss2.esp 	pi= 6	po= 9	nodes= 13	latches= 4
lits(sop)= 236	#states(STG)=  14
sis> Combinational power estimation, with Zero delay model.
Network: ex4.kiss2.esp, Power = 971.7 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- ex5 --> 
sis> sis> ex5.kiss2.esp 	pi= 2	po= 2	nodes=  4	latches= 2
lits(sop)=  28	#states(STG)=   4
sis> Combinational power estimation, with Zero delay model.
Network: ex5.kiss2.esp, Power = 189.2 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- ex6 --> 
sis> sis> ex6.kiss2.esp 	pi= 5	po= 8	nodes= 11	latches= 3
lits(sop)= 408	#states(STG)=   8
sis> Combinational power estimation, with Zero delay model.
Network: ex6.kiss2.esp, Power = 1436.9 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- ex7 --> 
sis> sis> ex7.kiss2.esp 	pi= 2	po= 2	nodes=  4	latches= 2
lits(sop)=  37	#states(STG)=   4
sis> Combinational power estimation, with Zero delay model.
Network: ex7.kiss2.esp, Power = 244.7 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- keyb --> 
sis> sis> keyb.kiss2.esp	pi= 7	po= 2	nodes=  7	latches= 5
lits(sop)=1156	#states(STG)=  19
sis> Combinational power estimation, with Zero delay model.
Network: keyb.kiss2.esp, Power = 3308.9 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- lion9 --> 
sis> sis> lion9.kiss2.esp	pi= 2	po= 1	nodes=  3	latches= 2
lits(sop)=  19	#states(STG)=   4
sis> Combinational power estimation, with Zero delay model.
Network: lion9.kiss2.esp, Power = 145.8 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- lion --> 
sis> sis> lion.kiss2.esp	pi= 2	po= 1	nodes=  3	latches= 2
lits(sop)=  23	#states(STG)=   4
sis> Combinational power estimation, with Zero delay model.
Network: lion.kiss2.esp, Power = 176.1 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- mark1 --> 
sis> sis> mark1.kiss2.esp	pi= 5	po=16	nodes= 20	latches= 4
lits(sop)= 237	#states(STG)=  12
sis> Combinational power estimation, with Zero delay model.
Network: mark1.kiss2.esp, Power = 921.8 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- mc --> 
sis> sis> mc.kiss2.esp  	pi= 3	po= 5	nodes=  7	latches= 2
lits(sop)=  54	#states(STG)=   4
sis> Combinational power estimation, with Zero delay model.
Network: mc.kiss2.esp, Power = 278.8 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- opus --> 
sis> sis> opus.kiss2.esp	pi= 5	po= 6	nodes= 10	latches= 4
lits(sop)= 272	#states(STG)=   9
sis> Combinational power estimation, with Zero delay model.
Network: opus.kiss2.esp, Power = 1133.6 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- planet1 --> 
sis> sis> planet1.kiss2.esp	pi= 7	po=19	nodes= 25	latches= 6
lits(sop)=2772	#states(STG)=  48
sis> Combinational power estimation, with Zero delay model.
Network: planet1.kiss2.esp, Power = 7832.4 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- planet --> 
sis> sis> planet.kiss2.esp	pi= 7	po=19	nodes= 25	latches= 6
lits(sop)=2772	#states(STG)=  48
sis> Combinational power estimation, with Zero delay model.
Network: planet.kiss2.esp, Power = 7832.4 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- s1488 --> 
sis> sis> s1488.kiss2.esp	pi= 8	po=19	nodes= 25	latches= 6
lits(sop)=2655	#states(STG)=  48
sis> Combinational power estimation, with Zero delay model.
Network: s1488.kiss2.esp, Power = 6946.4 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- s1494 --> 
sis> sis> s1494.kiss2.esp	pi= 8	po=19	nodes= 25	latches= 6
lits(sop)=2943	#states(STG)=  48
sis> Combinational power estimation, with Zero delay model.
Network: s1494.kiss2.esp, Power = 7690.5 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- s1 --> 
sis> sis> s1.kiss2.esp  	pi= 8	po= 6	nodes= 11	latches= 5
lits(sop)=1755	#states(STG)=  20
sis> Combinational power estimation, with Zero delay model.
Network: s1.kiss2.esp, Power = 4854.0 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- s208 --> 
sis> sis> s208.kiss2.esp	pi=11	po= 2	nodes=  7	latches= 5
lits(sop)= 145	#states(STG)=  18
sis> Combinational power estimation, with Zero delay model.
Network: s208.kiss2.esp, Power = 574.4 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- s27 --> 
sis> sis> s27.kiss2.esp 	pi= 4	po= 1	nodes=  4	latches= 3
lits(sop)=  49	#states(STG)=   5
sis> Combinational power estimation, with Zero delay model.
Network: s27.kiss2.esp, Power = 278.4 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- s298 --> 
sis> sis> s298.kiss2.esp	pi= 3	po= 6	nodes= 14	latches= 8
lits(sop)=7003	#states(STG)= 135
sis> Combinational power estimation, with Zero delay model.
Network: s298.kiss2.esp, Power = 19772.6 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- s386 --> 
sis> sis> s386.kiss2.esp	pi= 7	po= 7	nodes= 11	latches= 4
lits(sop)= 344	#states(STG)=  13
sis> Combinational power estimation, with Zero delay model.
Network: s386.kiss2.esp, Power = 1175.7 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- s420 --> 
sis> sis> s420.kiss2.esp	pi=19	po= 2	nodes=  7	latches= 5
lits(sop)= 145	#states(STG)=  18
sis> Combinational power estimation, with Zero delay model.
Network: s420.kiss2.esp, Power = 574.4 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- s510 --> 
sis> sis> s510.kiss2.esp	pi=19	po= 7	nodes= 13	latches= 6
lits(sop)=1043	#states(STG)=  47
sis> Combinational power estimation, with Zero delay model.
Network: s510.kiss2.esp, Power = 3133.7 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- s820 --> 
sis> sis> s820.kiss2.esp	pi=18	po=19	nodes= 24	latches= 5
lits(sop)= 849	#states(STG)=  24
sis> Combinational power estimation, with Zero delay model.
Network: s820.kiss2.esp, Power = 2306.8 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- s832 --> 
sis> sis> s832.kiss2.esp	pi=18	po=19	nodes= 24	latches= 5
lits(sop)= 857	#states(STG)=  24
sis> Combinational power estimation, with Zero delay model.
Network: s832.kiss2.esp, Power = 2323.0 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- sand --> 
sis> sis> sand.kiss2.esp	pi=11	po= 9	nodes= 14	latches= 5
lits(sop)=2560	#states(STG)=  32
sis> Combinational power estimation, with Zero delay model.
Network: sand.kiss2.esp, Power = 6840.5 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- shiftreg --> 
sis> sis> shiftreg.kiss2.esp	pi= 1	po= 1	nodes=  4	latches= 3
lits(sop)=  18	#states(STG)=   8
sis> Combinational power estimation, with Zero delay model.
Network: shiftreg.kiss2.esp, Power = 148.8 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- sse --> 
sis> sis> sse.kiss2.esp 	pi= 7	po= 7	nodes= 11	latches= 4
lits(sop)= 299	#states(STG)=  13
sis> Combinational power estimation, with Zero delay model.
Network: sse.kiss2.esp, Power = 1055.3 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- styr --> 
sis> sis> styr.kiss2.esp	pi= 9	po=10	nodes= 15	latches= 5
lits(sop)=2029	#states(STG)=  30
sis> Combinational power estimation, with Zero delay model.
Network: styr.kiss2.esp, Power = 5302.7 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- tav --> 
sis> sis> tav.kiss2.esp 	pi= 4	po= 4	nodes=  6	latches= 2
lits(sop)=  35	#states(STG)=   4
sis> Combinational power estimation, with Zero delay model.
Network: tav.kiss2.esp, Power = 200.9 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- tbk --> 
sis> sis> tbk.kiss2.esp 	pi= 6	po= 3	nodes=  7	latches= 4
lits(sop)= 993	#states(STG)=  16
sis> Combinational power estimation, with Zero delay model.
Network: tbk.kiss2.esp, Power = 2527.5 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- train11 --> 
sis> sis> train11.kiss2.esp	pi= 2	po= 1	nodes=  3	latches= 2
lits(sop)=  27	#states(STG)=   4
sis> Combinational power estimation, with Zero delay model.
Network: train11.kiss2.esp, Power = 179.3 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
sis> <-- START --> 
sis> sis> <-- train4 --> 
sis> sis> train4.kiss2.esp	pi= 2	po= 1	nodes=  3	latches= 2
lits(sop)=  29	#states(STG)=   4
sis> Combinational power estimation, with Zero delay model.
Network: train4.kiss2.esp, Power = 185.4 uW assuming 20 MHz clock and Vdd = 5V
sis> <-- END --> 
