 
   July 1, 1994                                                        SIS(1)
 
   one_hot
 
     Does a quick one-hot encoding of the current STG.  It assigns one-hot
     codes, minimizes the resulting PLA using espresso, and returns the net-
     work to SIS.
 
                                                                            1
