.\" /*
.\"  * Revision Control Information
.\"  *
.\"  * $Source$
.\"  * $Author$
.\"  * $Revision$
.\"  * $Date$
.\"  *
.\"
.XX
force_init_0
.PP
This command replaces all latches initialized to 1 by latches
initialized to 0. It inserts an inverter before and after the latch
to maintain circuit behavior. 
.PP
This command is useful for certain types of FPGA architectures
which do not support the initialization of latches to 1.
