.\" /*
.\"  * Revision Control Information
.\"  *
.\"  * $Source: /vol/opua/opua2/sis/sis-1.1/common/src/sis/sis_lib/help/RCS/tech_decomp.1,v $
.\"  * $Author: sis $
.\"  * $Revision: 1.2 $
.\"  * $Date: 1992/05/06 19:04:01 $
.\"  *
.\"
.XX
tech_decomp [-a and-limit] [-o or-limit] 
.PP
Decompose all the nodes in the current network into AND gates
or OR gates or both depending on whether \fB-a\fR,
\fB-o\fR, or both flags are specified.
The fanins of AND gates
will be no more than \fBand-limit\fR and that of the OR gates
will be no more than \fBor-limit\fR.  \fBand-limit\fR and
\fBor-limit\fR, if specified, must be at least 2.
The default option is \fB-a 2\fR.
