.\" /*
.\"  * Revision Control Information
.\"  *
.\"  * $Source: /vol/opua/opua2/sis/sis-1.1/common/src/sis/sis_lib/help/RCS/print_library.1,v $
.\"  * $Author: sis $
.\"  * $Revision: 1.2 $
.\"  * $Date: 1992/05/06 19:04:01 $
.\"  *
.\"
.XX
print_library [-a][-f][-h][-l][-r] [function-string]
.PP
Print the contents of the current library.  If the optional string is
given, only the combinational gates with the same logic function as the string
will be printed.  \fIfunction-string\fP is in the format of
read_eqn.  For example
.in +1i
.nf
print_library "f=!(a*b);" 
.in -1i
.fi
will print all combinational gates with a NAND2 logic function.
.PP
The \fB-a\fP option prints asynchronous type latches matching the 'function-string'.
.PP
The \fB-f\fP option prints falling edge triggered flip-flops matching the 'function-string'.
.PP
The \fB-h\fP option prints active high transparent latches matching the 'function-string'.
.PP
The \fB-l\fP option prints active low transparent latches matching the 'function-string'.
.PP
The \fB-r\fP option prints rising edge triggered flip-flops matching the 'function-string'.

