 
   July 1, 1994                                                        SIS(1)
 
   print_library [-a][-f][-h][-l][-r] [function-string]
 
     Print the contents of the current library.  If the optional string is
     given, only the combinational gates with the same logic function as the
     string will be printed.  function-string is in the format of read_eqn.
     For example
               print_library "f=!(a*b);"
     will print all combinational gates with a NAND2 logic function.
 
     The -a option prints asynchronous type latches matching the 'function-
     string'.
 
     The -f option prints falling edge triggered flip-flops matching the
     'function-string'.
 
     The -h option prints active high transparent latches matching the
     'function-string'.
 
     The -l option prints active low transparent latches matching the
     'function-string'.
 
     The -r option prints rising edge triggered flip-flops matching the
     'function-string'.
 
                                                                            1
