.\" /*
.\"  * Revision Control Information
.\"  *
.\"  * $Source: /vol/opua/opua2/sis/sis-1.1/common/src/sis/sis_lib/help/RCS/write_pds.1,v $
.\"  * $Author: sis $
.\"  * $Revision: 1.2 $
.\"  * $Date: 1992/05/06 19:04:01 $
.\"  *
.\"
.XX
write_pds [-c] [-d] [-s] [filename]
.PP
Write the current network to file \fBfilename\fP in the \fIpds\fP
format suitable for Xilinx.  
The \fIpds\fP descriptions are generated for single output CLBs
(LUTs) only.
.PP
The \fB-c\fP option indicates that only the combinational portion
of the network should be written out.
.PP
The \fB-d\fP option will cause debugging information to be printed.
.PP
The \fB-s\fP option uses the network short names rather than the
network long names for the \fIpds\fP file.
